Janatics pneumatics:

Official site- www.janatics.com

Thin pneumatic cylinders-

Model:

A51, A52 series- Air cylinder Double Acting (ISO 6432/ CETOP RP52P standards)

Features:

1. Elastomer cushioning at both ends

2. Wide varieties of mountings

3. Long life

4. Low friction

Technical specifications:

Cylinder bore- 8-10mm

Std. strokes- 10, 25, 40, 50, 80, 100mm

Medium- Compressed air-filtered-lubricated

Working pressure- 0.5-10bars

Medium temp- 5-60(degree Celsius)

Mountings- Front foot mounting, double foot mounting, front flange, rear flange, front trunnion, rear trunnion etc.

Accessories- Clevis foot bracket Rod end fork

Address:

Mumbai 1-

603, Thacker towers, Plot no. 86, Sector-17, Vashi, Navi Mumbai-400075

Tel- 022-27891276

Fax- 022-67913967

Mob- 98202 31744

Mumbai 2-

8/35, Ajanta House, Marol Co-op Industrial Estate, MV Road, Marol, Andheri East, Mumbai-400059

Tel- 022-28560894

Mob- 7738760177

Email- janatics\_mum2@janatics.co.in

For further details, visit: www.janatics.com